 Caption = Shear Walls
 Editable = True
Created = 02-01-02 
Revision Date = 
-------------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Hollow Shear Wall
  Category = Cross Section
  Basic Shape Type = Rectangular
  Sub Shape Type = Rectangular
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 2
 Nb = 2
 Nh = 2
 Ncord = 8
  
 Path Data
 1             4             1
 5             8            -1
  
 Horizontal Data
 B1=72
 B2=8
  
 Vertical Data
 H1=72
 H2=8
  
 X Data
 X1=0
 X2=0
 X3=B1
 X4=B1
 X5=B2
 X6=B2
 X7=B1-B2
 X8=B1-B2

  
 Y Data
 Y1=0
 Y2=H1
 Y3=H1
 Y4=0
 Y5=H2
 Y6=H1-H2
 Y7=H1-H2
 Y8=H2
  
 Horizontal Dimension
<Dimension Notations>
"        C-b","2","3","2"
"       L-t1","1","5","1"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","2","-1"
"       R-t2","4","8","1"
  
 Tessellation
 1
          1/4
  
 Line Data
 <Line Notation>
 4             4 
  
 Line X Data
          X1=B2/2
          X2=B2/2
          X3=B1-B2/2
          X4=B1-B2/2
  
 Line Y Data
          Y1=H2/2
          Y2=H1-H2/2
          Y3=H1-H2/2
          Y4=H2/2
  
 Line Thickness
 2
          T1=t2
          T2=t2
  
 Line Connectivity Data
 <Conectivity Notation>
"          1","2","T1"
"          2","3","T2"
"          3","4","T2"
"          4","1","T1"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = C Shear Wall
  Category = Cross Section
  Basic Shape Type = C Shaped
  Sub Shape Type = C Shaped
  Is Hollow = No
  Is Champher = No
  Is Fillet = Yes
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 3
 Nh = 1
 Ncord = 12
  
 Path Data
 1             12            1 
  
 Horizontal Data
 B1=72
 B2=20
 B3=8
  
 Vertical Data
 H1=72
  
 X Data
 X1=B1/2-B2/2
 X2=0
 X3=0
 X4=B1
 X5=B1
 X6=B1/2+B2/2
 X7=B1/2+B2/2
 X8=B1-B3
 X9=B1-B3
 X10=B3
 X11=B3
 X12=B1/2-B2/2
  
 Y Data
 Y1=0
 Y2=0
 Y3=H1
 Y4=H1
 Y5=0
 Y6=0
 Y7=B3
 Y8=B3
 Y9=H1-B3
 Y10=H1-B3
 Y11=B3
 Y12=B3
  
 Horizontal Dimension
<Dimension Notations>
"        C-bf","2","5","1"
"        C-b2","1","6","-1"
"          L-t","8","5","-1"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","2","3","-1"
  
 Tessellation
 7
         1,2,3,24
         24,3,4,17,18,21
         21,18,19,20
         4,5,16,17
         5,6,9,12,15,16
         6/9
         12/15
  
 Line Data
 <Line Notation>
 5            6 
  
 Line X Data
         X1=B1/2-B2/2
         X2=B3/2
         X3=B3/2
         X4=B1-B3/2
         X5=B1-B3/2
         X6=B1/2+B2/2
  
 Line Y Data
         Y1=B3/2
         Y2=B3/2
         Y3=H1-B3/2
         Y4=H1-B3/2
         Y5=B3/2
         Y6=B3/2
  
 Line Thickness
 1
         T1=B3
  
 Line Connectivity Data
 <Conectivity Notation>
"         1","2","T1"
"         2","3","T1"
"         3","4","T1"
"         4","5","T1"
"         5","6","T1"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
  NEW SHAPE
 
 TYPE = ShapeGeneral
  Caption = Double C Shear Wall
  Category = Cross section
  Basic Shape Type = Double C
  Sub Shape Type = Double C
  Is Hollow = Yes
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete  
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = Yes

 Control Data
 Np=1
 Nb=3
 Nh=1
 Ncord=20

 Path Data
 1,20,1

 Horizontal Data
 B1=144
 B2=30
 B3=8

 Vertical Data
 H1=72

 X Data
 X1=B1/4-B2/2
 X2=0
 X3=0
 X4=B1
 X5=B1
 X6=3*B1/4+B2/2
 X7=3*B1/4+B2/2
 X8=B1-B3
 X9=B1-B3
 X10=B1/2+B3/2
 X11=B1/2+B3/2
 X12=B1/2+B2/2
 X13=B1/2+B2/2
 X14=B1/2-B2/2
 X15=B1/2-B2/2
 X16=B1/2-B3/2
 X17=B1/2-B3/2
 X18=B3
 X19=B3
 X20=B1/4-B2/2

 Y Data
 Y1=0
 Y2=0
 Y3=H1
 Y4=H1
 Y5=0
 Y6=0
 Y7=B3
 Y8=B3
 Y9=H1-B3
 Y10=H1-B3
 Y11=B3
 Y12=B3
 Y13=0
 Y14=0
 Y15=B3
 Y16=B3
 Y17=H1-B3
 Y18=H1-B3
 Y19=B3
 Y20=B3

 Horizontal Dimension
"Dimension Name","First Pt", "Second Pt","Scal"
 "        C-b","3","4","1"
 "        C-b1","1","14","-1"
 "        L-t","8","5","-1"

 Vertical Dimension
"Dimension Name","First Pt", "Second Pt","Scal"
 "        C-h","2","3","-1"

 Tessellation
 24
 1,2,26,25
 2,3,27,26
 3,4,28,27
 4,5,29,28
 5,6,30,29
 6,7,31,30
 7,8,32,31
 8,9,33,32
 9,10,34,33
 10,11,35,34
 11,12,36,35
 12,13,37,36
 13,14,38,37
 14,15,39,38
 15,16,40,39
 16,17,41,40
 17,18,42,41
 18,19,43,42
 19,20,44,43
 20,21,45,44
 21,22,46,45
 22,23,47,46
 23,24,48,47
 24,1,25,48

 Line Data
 "No Lines","No of Nodes"
 9,10

 Line X Data
 X1=B1/4-B2/2
 X2=B3/2
 X3=B3/2
 X4=B1/2
 X5=B1-B3/2
 X6=B1-B3/2
 X7=3*B1/4+B2/2
 X8=B1/2+B2/2
 X9=B1/2
 X10=B1/2-B2/2

Line Y Data
 Y1=B3/2
 Y2=B3/2
 Y3=H1-B3/2
 Y4=H1-B3/2
 Y5=H1-B3/2
 Y6=B3/2
 Y7=B3/2
 Y8=B3/2
 Y9=B3/2
 Y10=B3/2

 Line Thickness
 1
 T1=B3

 Line Connectivity Data
"Nodei","Nodej",Thickness
 1,2,T1
 2,3,T1
 3,4,T1
 4,5,T1
 5,6,T1
 6,7,T1
 8,9,T1
 9,10,T1
 9,4,T1
 Prop From Database=No
 Prop Database=None
 Prop Record No=0

 TAG = 
 END TYPE = ShapeGeneral

 END SHAPE

 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Box Shape With Two Core
  Category = Cross section
  Basic Shape Type = Rectangular
  Sub Shape Type = Box
  Is Hollow = Yes
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 3
 Nb = 3
 Nh = 1
 Ncord = 12
  
 Path Data
 1             4             1 
 5             8            -1
 9           12           -1
  
 Horizontal Data
 B1=144
 B2=6
 B3=8
  
 Vertical Data
 H1=72
  
 X Data
 X1=0
 X2=0
 X3=B1
 X4=B1
 X5=B3
 X6=B3
 X7=B1/2-B2/2
 X8=B1/2-B2/2
 X9=B1/2+B2/2
 X10=B1/2+B2/2
 X11=B1-B3
 X12=B1-B3
  
 Y Data
 Y1=0
 Y2=H1
 Y3=H1
 Y4=0
 Y5=B3
 Y6=H1-B3
 Y7=H1-B3
 Y8=B3
 Y9=B3
 Y10=H1-B3
 Y11=H1-B3
 Y12=B3
  
 Horizontal Dimension
<Dimension Notations>
"        C-b1","1","4","1"
"        L-t1","8","9","-1"
"        L-t2","12","4","-1"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","2","-1"
  
 Tessellation
 4
2,3,11,10,9,1
4,5,13,12,11,3
6,7,15,14,13,5
8,1,9,16,15,7

Line Data
"No Lines","No of Nodes"
 7,6

 Line X Data
 X1=B3/2
 X2=B3/2
 X3=B1/2
 X4=B1-B3/3
 X5=B1-B3/2
 X6=B1/2

Line Y Data
 Y1=B3/2
 Y2=H1-B3/2
 Y3=H1-B3/2
 Y4=H1-B3/2
 Y5=B3/2
 Y6=B3/2

 Line Thickness
 2
 T1=B3
 T2=B2

 Line Connectivity Data
"Nodei","Nodej",Thickness
 1,2,T1
 2,3,T1
 3,4,T1
 4,5,T1
 5,6,T1
 6,1,T1
 6,3,T2
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Box Shape With Three Core
  Category = Cross section
  Basic Shape Type = Rectangular
  Sub Shape Type = Box
  Is Hollow = Yes
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 4
 Nb = 3
 Nh = 1
 Ncord = 16
  
 Path Data
 1             4             1 
 5             8            -1
 9           12            -1
13          16           -1
  
 Horizontal Data
 B1=144
 B2=6
 B3=8
  
 Vertical Data
 H1=72
  
 X Data
 X1=0
 X2=0
 X3=B1
 X4=B1
 X5=B3
 X6=B3
 X7=B3+(B1-2*B2-2*B3)/3
 X8=B3+(B1-2*B2-2*B3)/3
 X9=B3+(B1-2*B2-2*B3)/3+B2
 X10=B3+(B1-2*B2-2*B3)/3+B2
 X11=B3+2*(B1-2*B2-2*B3)/3+B2
 X12=B3+2*(B1-2*B2-2*B3)/3+B2
 X13=B3+2*(B1-2*B2-2*B3)/3+B2+B2
 X14=B3+2*(B1-2*B2-2*B3)/3+B2+B2
 X15=B1-B3
 X16=B1-B3
  
 Y Data
 Y1=0
 Y2=H1
 Y3=H1
 Y4=0
 Y5=B3
 Y6=H1-B3
 Y7=H1-B3
 Y8=B3
 Y9=B3
 Y10=H1-B3
 Y11=H1-B3
 Y12=B3
 Y13=B3
 Y14=H1-B3
 Y15=H1-B3
 Y16=B3
  
 Horizontal Dimension
<Dimension Notations>
"        C-b1","1","4","1"
"        L-t1","8","9","-1"
"        L-t2","16","4","-1"
  
 Vertical Dimension
<Dimension Notations>
"        C-h1","1","2","-1"
  
 Tessellation
 4
2,3,11,10,9,1
4,5,13,12,11,3
6,7,15,14,13,5
8,1,9,16,15,7

Line Data
"No Lines","No of Nodes"
 10,8

 Line X Data
 X1=B3/2
 X2=B3/2
 X3=B3+(B1-2*B2-2*B3)/3+B2/2
 X4=B3+2*(B1-2*B2-2*B3)/3+B2+B2/2
 X5=B1-B3/2
 X6=B1-B3/2
 X7=B3+2*(B1-2*B2-2*B3)/3+B2+B2/2
 X8=B3+(B1-2*B2-2*B3)/3+B2/2

Line Y Data
 Y1=B3/2
 Y2=H1-B3/2
 Y3=H1-B3/2
 Y4=H1-B3/2
 Y5=H1-B3/2
 Y6=B3/2
 Y7=B3/2
 Y8=B3/2

 Line Thickness
 2
 T1=B3
 T2=B2

 Line Connectivity Data
"Nodei","Nodej",Thickness
 1,2,T1
 2,3,T1
 3,4,T1
 4,5,T1
 5,6,T1
 6,7,T1
 7,8,T1
 8,1,T1
 7,4,T2
 8,3,T2
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
