 Caption = Basic Concrete Shapes
 Editable = False
 Revision Date = 27-7-01 Last Changes in tessellation of I section
-------------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Rectangular Shape
  Category = Cross Section
  Basic Shape Type = Rectangular
  Sub Shape Type = Rectangular
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 1
 Nh = 1
 Ncord = 4
  
 Path Data
 1             4             1 
  
 Horizontal Data
 B1=24
  
 Vertical Data
 H1=36
  
 X Data
 X1=0
 X2=0
 X3=B1
 X4=B1
  
 Y Data
 Y1=0
 Y2=H1
 Y3=H1
 Y4=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-b","2","3","1"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","2","-1"
  
 Tessellation
 1
          1/4
  
 Line Data
 <Line Notation>
 2             3 
  
 Line X Data
          X1=B1/2
          X2=B1/2
          X3=B1/2
  
 Line Y Data
          Y1=0
          Y2=H1/2
          Y3=H1
  
 Line Thickness
 1
          T1=B1
  
 Line Connectivity Data
 <Conectivity Notation>
"          1","2","T1"
"          2","3","T1"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Fillet I Shape
  Category = Cross Section
  Basic Shape Type = Flanged
  Sub Shape Type = Fillet Flanged
  Is Hollow = No
  Is Champher = No
  Is Fillet = Yes
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 7
 Nh = 5
 Ncord = 24
  
 Path Data
 1             24            1 
  
 Horizontal Data
 B1=36
 B2=24
 B3=4
 B4=4
 B5=4
 B6=4
 B7=8
  
 Vertical Data
 H1=36
 H2=6
 H3=6
 H4=2
 H5=2
  
 X Data
 X1=B1/2-B2/2
 X2=B1/2-B2/2
 X3=B1/2-B7/2-B3
 X4=B1/2-B7/2
 X5=B1/2-B7/2
 X6=B1/2-B7/2-B4
 X7=0
 X8=0
 X9=B1/2-B7/2-B4
 X10=B1/2-B7/2
 X11=B1/2+B7/2
 X12=B1/2+B7/2+B5
 X13=B1
 X14=B1
 X15=B1/2+B7/2+B5
 X16=B1/2+B7/2
 X17=B1/2+B7/2
 X18=B1/2+B7/2+B6
 X19=B1/2+B2/2
 X20=B1/2+B2/2
 X21=B1/2+B7/2+B6
 X22=B1/2+B7/2
 X23=B1/2-B7/2
 X24=B1/2-B7/2-B3
  
 Y Data
 Y1=0
 Y2=H3
 Y3=H3
 Y4=H3+H4
 Y5=H1-H2-H5
 Y6=H1-H2
 Y7=H1-H2
 Y8=H1
 Y9=H1
 Y10=H1
 Y11=H1
 Y12=H1
 Y13=H1
 Y14=H1-H2
 Y15=H1-H2
 Y16=H1-H2-H5
 Y17=H3+H4
 Y18=H3
 Y19=H3
 Y20=0
 Y21=0
 Y22=0
 Y23=0
 Y24=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-bf(top)","8","13","2"
"        C-bf(bot)","1","20","-2"
"        L-b1","3","4","-1"
"        L-b2","5","6","1"
"        R-b3","15","16","1"
"        L-b4","17","18","-1"
"        C-tw","4","17","0.6H"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","8","-2"
"        L-tf1","13","14","1"
"        R-tf2","19","20","1"
"        R-f1","3","4","-1"
"        L-f2","5","6","-1"
  
 Tessellation
 7
         1,2,3,24
         24,3,4,17,18,21
         21,18,19,20
         4,5,16,17
         5,6,9,12,15,16
         6/9
         12/15
  
 Line Data
 <Line Notation>
 10            11 
  
 Line X Data
         X1=B1/2-B2/2
         X2=B1/2-B3-B7/2
         X3=B1/2
         X4=B1/2+B3+B7/2
         X5=B1/2+B2/2
         X6=B1/2
         X7=0
         X8=B1/2-B4-B7/2
         X9=B1/2
         X10=B1/2+B4+B7/2
         X11=B1
  
 Line Y Data
         Y1=H3/2
         Y2=H3/2
         Y3=(H3+H4)/2
         Y4=H3/2
         Y5=H3/2
         Y6=H1/2
         Y7=H1-H2/2
         Y8=H1-H2/2
         Y9=H1-(H2+H5)/2
         Y10=H1-H2/2
         Y11=H1-H2/2
  
 Line Thickness
 10
         T1=H3
         T2=(H3+H4)/2
         T3=(H3+H4)/2
         T4=H3
         T5=B7
         T6=B7
         T7=H2
         T8=(H2+H5)/2
         T9=(H2+H5)/2
         T10=H2
  
 Line Connectivity Data
 <Conectivity Notation>
"         1","2","T1"
"         2","3","T2"
"         3","4","T3"
"         4","5","T4"
"         3","6","T5"
"         6","9","T6"
"         7","8","T7"
"         8","9","T8"
"         9","10","T9"
"         10","11","T10"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
  NEW SHAPE
 
 TYPE = ShapeGeneral
  Caption = Hollow Circle
  Category = Cross section
  Basic Shape Type = Circular
  Sub Shape Type = Pipe
  Is Hollow = Yes
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete  
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = Yes

 Control Data
 Np=2
 Nb=2
 Nh=0
 Ncord=48

 Path Data
 1,24,1
 25,48,-1

 Horizontal Data
 B1=30
 B2=6

 Vertical Data

 X Data
 X1=0
 X2=B1/2-B1/2*0.9659
 X3=B1/2-B1/2*0.8660
 X4=B1/2-B1/2*0.7071
 X5=B1/2-B1/2*0.5
 X6=B1/2-B1/2*0.2588
 X7=B1/2
 X8=B1/2+B1/2*0.2588
 X9=B1/2+B1/2*0.5
 X10=B1/2+B1/2*0.7071
 X11=B1/2+B1/2*0.8660
 X12=B1/2+B1/2*0.9659
 X13=B1/2+B1/2
 X14=B1/2+B1/2*0.9659
 X15=B1/2+B1/2*0.8660
 X16=B1/2+B1/2*0.7071
 X17=B1/2+B1/2*0.5
 X18=B1/2+B1/2*0.2588
 X19=B1/2
 X20=B1/2-B1/2*0.2588
 X21=B1/2-B1/2*0.5
 X22=B1/2-B1/2*0.7071
 X23=B1/2-B1/2*0.8660
 X24=B1/2-B1/2*0.9659
 X25=B2
 X26=B1/2-(B1/2-B2)*0.9659
 X27=B1/2-(B1/2-B2)*0.8660
 X28=B1/2-(B1/2-B2)*0.7071
 X29=B1/2-(B1/2-B2)*0.5
 X30=B1/2-(B1/2-B2)*0.2588
 X31=B1/2
 X32=B1/2+(B1/2-B2)*0.2588
 X33=B1/2+(B1/2-B2)*0.5
 X34=B1/2+(B1/2-B2)*0.7071
 X35=B1/2+(B1/2-B2)*0.8660
 X36=B1/2+(B1/2-B2)*0.9659
 X37=B1/2+(B1/2-B2)
 X38=B1/2+(B1/2-B2)*0.9659
 X39=B1/2+(B1/2-B2)*0.8660
 X40=B1/2+(B1/2-B2)*0.7071
 X41=B1/2+(B1/2-B2)*0.5
 X42=B1/2+(B1/2-B2)*0.2588
 X43=B1/2
 X44=B1/2-(B1/2-B2)*0.2588
 X45=B1/2-(B1/2-B2)*0.5
 X46=B1/2-(B1/2-B2)*0.7071
 X47=B1/2-(B1/2-B2)*0.8660
 X48=B1/2-(B1/2-B2)*0.9659

 Y Data
 Y1=B1/2
 Y2=B1/2+B1/2*0.2588
 Y3=B1/2+B1/2*0.5
 Y4=B1/2+B1/2*0.7071
 Y5=B1/2+B1/2*0.8660
 Y6=B1/2+B1/2*0.9659
 Y7=B1/2+B1/2
 Y8=B1/2+B1/2*0.9659
 Y9=B1/2+B1/2*0.8660
 Y10=B1/2+B1/2*0.7071
 Y11=B1/2+B1/2*0.5
 Y12=B1/2+B1/2*0.2588
 Y13=B1/2
 Y14=B1/2-B1/2*0.2588
 Y15=B1/2-B1/2*0.5
 Y16=B1/2-B1/2*0.7071
 Y17=B1/2-B1/2*0.8660
 Y18=B1/2-B1/2*0.9659
 Y19=0
 Y20=B1/2-B1/2*0.9659
 Y21=B1/2-B1/2*0.8660
 Y22=B1/2-B1/2*0.7071
 Y23=B1/2-B1/2*0.5
 Y24=B1/2-B1/2*0.2588
 Y25=B1/2
 Y26=B1/2+(B1/2-B2)*0.2588
 Y27=B1/2+(B1/2-B2)*0.5
 Y28=B1/2+(B1/2-B2)*0.7071
 Y29=B1/2+(B1/2-B2)*0.8660
 Y30=B1/2+(B1/2-B2)*0.9659
 Y31=B1/2+(B1/2-B2)
 Y32=B1/2+(B1/2-B2)*0.9659
 Y33=B1/2+(B1/2-B2)*0.8660
 Y34=B1/2+(B1/2-B2)*0.7071
 Y35=B1/2+(B1/2-B2)*0.5
 Y36=B1/2+(B1/2-B2)*0.2588
 Y37=B1/2
 Y38=B1/2-(B1/2-B2)*0.2588
 Y39=B1/2-(B1/2-B2)*0.5
 Y40=B1/2-(B1/2-B2)*0.7071
 Y41=B1/2-(B1/2-B2)*0.8660
 Y42=B1/2-(B1/2-B2)*0.9659
 Y43=B2
 Y44=B1/2-(B1/2-B2)*0.9659
 Y45=B1/2-(B1/2-B2)*0.8660
 Y46=B1/2-(B1/2-B2)*0.7071
 Y47=B1/2-(B1/2-B2)*0.5
 Y48=B1/2-(B1/2-B2)*0.2588

 Horizontal Dimension
"Dimension Name","First Pt", "Second Pt","Scal"
 "        C-Dia","1","13","1"
 "        R-t","1","25","0.5H"

 Vertical Dimension
"Dimension Name","First Pt", "Second Pt","Scal"

 Tessellation
 24
 1,2,26,25
 2,3,27,26
 3,4,28,27
 4,5,29,28
 5,6,30,29
 6,7,31,30
 7,8,32,31
 8,9,33,32
 9,10,34,33
 10,11,35,34
 11,12,36,35
 12,13,37,36
 13,14,38,37
 14,15,39,38
 15,16,40,39
 16,17,41,40
 17,18,42,41
 18,19,43,42
 19,20,44,43
 20,21,45,44
 21,22,46,45
 22,23,47,46
 23,24,48,47
 24,1,25,48

 Line Data
 "No Lines","No of Nodes"
 24,24

 Line X Data
 X1=B2/2
 X2=B1/2-(B1/2-B2/2)*0.9659
 X3=B1/2-(B1/2-B2/2)*0.8660
 X4=B1/2-(B1/2-B2/2)*0.7071
 X5=B1/2-(B1/2-B2/2)*0.5
 X6=B1/2-(B1/2-B2/2)*0.2588
 X7=B1/2
 X8=B1/2+(B1/2-B2/2)*0.2588
 X9=B1/2+(B1/2-B2/2)*0.5
 X10=B1/2+(B1/2-B2/2)*0.7071
 X11=B1/2+(B1/2-B2/2)*0.8660
 X12=B1/2+(B1/2-B2/2)*0.9659
 X13=B1/2+(B1/2-B2/2)
 X14=B1/2+(B1/2-B2/2)*0.9659
 X15=B1/2+(B1/2-B2/2)*0.8660
 X16=B1/2+(B1/2-B2/2)*0.7071
 X17=B1/2+(B1/2-B2/2)*0.5
 X18=B1/2+(B1/2-B2/2)*0.2588
 X19=B1/2
 X20=B1/2-(B1/2-B2/2)*0.2588
 X21=B1/2-(B1/2-B2/2)*0.5
 X22=B1/2-(B1/2-B2/2)*0.7071
 X23=B1/2-(B1/2-B2/2)*0.8660
 X24=B1/2-(B1/2-B2/2)*0.9659

Line Y Data
 Y1=B1/2
 Y2=B1/2+(B1/2-B2/2)*0.2588
 Y3=B1/2+(B1/2-B2/2)*0.5
 Y4=B1/2+(B1/2-B2/2)*0.7071
 Y5=B1/2+(B1/2-B2/2)*0.8660
 Y6=B1/2+(B1/2-B2/2)*0.9659
 Y7=B1/2+(B1/2-B2/2)
 Y8=B1/2+(B1/2-B2/2)*0.9659
 Y9=B1/2+(B1/2-B2/2)*0.8660
 Y10=B1/2+(B1/2-B2/2)*0.7071
 Y11=B1/2+(B1/2-B2/2)*0.5
 Y12=B1/2+(B1/2-B2/2)*0.2588
 Y13=B1/2
 Y14=B1/2-(B1/2-B2/2)*0.2588
 Y15=B1/2-(B1/2-B2/2)*0.5
 Y16=B1/2-(B1/2-B2/2)*0.7071
 Y17=B1/2-(B1/2-B2/2)*0.8660
 Y18=B1/2-(B1/2-B2/2)*0.9659
 Y19=B2/2
 Y20=B1/2-(B1/2-B2/2)*0.9659
 Y21=B1/2-(B1/2-B2/2)*0.8660
 Y22=B1/2-(B1/2-B2/2)*0.7071
 Y23=B1/2-(B1/2-B2/2)*0.5
 Y24=B1/2-(B1/2-B2/2)*0.2588

 Line Thickness
 1
 T1=B2

 Line Connectivity Data
"Nodei","Nodej",Thickness
 1,2,T1
 2,3,T1
 3,4,T1
 4,5,T1
 5,6,T1
 6,7,T1
 7,8,T1
 8,9,T1
 9,10,T1
 10,11,T1
 11,12,T1
 12,13,T1
 13,14,T1
 14,15,T1
 15,16,T1
 16,17,T1
 17,18,T1
 18,19,T1
 19,20,T1
 20,21,T1
 21,22,T1
 22,23,T1
 23,24,T1
 24,1,T1
 Prop From Database=No
 Prop Database=None
 Prop Record No=0

 TAG = 
 END TYPE = ShapeGeneral

 END SHAPE

 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Box Shape
  Category = Cross section
  Basic Shape Type = Rectangular
  Sub Shape Type = Box
  Is Hollow = Yes
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 2
 Nb = 2
 Nh = 2
 Ncord = 16
  
 Path Data
 1             8             1 
 9             16            -1 
  
 Horizontal Data
 B1=24
 B2=6
  
 Vertical Data
 H1=36
 H2=6
  
 X Data
 X1=0
 X2=0
 X3=0
 X4=B1/2
 X5=B1
 X6=B1
 X7=B1
 X8=B1/2
 X9=B2
 X10=B2
 X11=B2
 X12=B1/2
 X13=B1-B2
 X14=B1-B2
 X15=B1-B2
 X16=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1
 Y5=H1
 Y6=H1/2
 Y7=0
 Y8=0
 Y9=H2
 Y10=H1/2
 Y11=H1-H2
 Y12=H1-H2
 Y13=H1-H2
 Y14=H1/2
 Y15=H2
 Y16=H2
  
 Horizontal Dimension
<Dimension Notations>
"        C-t2","1","7","2"
"        R-tw","2","10","0.5H"
  
 Vertical Dimension
<Dimension Notations>
"        C-t3","1","3","-2"
"        R-tf","1","9","0.5B"
  
 Tessellation
 4
2,3,11,10,9,1
4,5,13,12,11,3
6,7,15,14,13,5
8,1,9,16,15,7

 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = L Shape
  Category = Cross section
  Basic Shape Type = Flanged
  Sub Shape Type = Angle
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 2
 Nh = 2
 Ncord = 10
  
 Path Data
 1             10            1 
  
 Horizontal Data
 B1=24
 B2=6
  
 Vertical Data
 H1=36
 H2=8
  
 X Data
 X1=0
 X2=0
 X3=0
 X4=B2
 X5=B2
 X6=B2
 X7=B2+(B1-B2)/2
 X8=B1
 X9=B1
 X10=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1
 Y5=H2+(H1-H2)/2
 Y6=H2
 Y7=H2
 Y8=H2
 Y9=0
 Y10=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-b","1","9","2"
"        R-tw","3","4","0.8H"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","3","-2"
"        R-tf","8","9","0.7B"

  
 Tessellation
 4
        1,2,5,6
        2,3,4,5
        1,6,7,10
        10,7,8,9
  
 Line Data
 <Line Notation>
 4             5 
  
 Line X Data
        X1=B2/2
        X2=B2/2
        X3=B2/2
        X4=B1/2
        X5=B1
  
 Line Y Data
        Y1=H1
        Y2=H1/2
        Y3=H2/2
        Y4=H2/2
        Y5=H2/2
  
 Line Thickness
 1
        T1=B2
  
 Line Connectivity Data
 <Conectivity Notation>
"        1","2","T1"
"        2","3","T1"
"        3","4","T1"
"        4","5","T1"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0

  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = T Shape
  Category = Cross section
  Basic Shape Type = Flanged
  Sub Shape Type = Tee
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 2
 Nh = 2
 Ncord = 11
  
 Path Data
 1             11            1 
  
 Horizontal Data
 B1=36
 B2=6
  
 Vertical Data
 H1=36
 H2=8
  
 X Data
 X1=B1/2-B2/2
 X2=B1/2-B2/2
 X3=B1/2-B2/2
 X4=0
 X5=0
 X6=B1/2
 X7=B1
 X8=B1
 X9=B1/2+B2/2
 X10=B1/2+B2/2
 X11=B1/2+B2/2
  
 Y Data
 Y1=0
 Y2=(H1-H2)/2
 Y3=H1-H2
 Y4=H1-H2
 Y5=H1
 Y6=H1
 Y7=H1
 Y8=H1-H2
 Y9=H1-H2
 Y10=(H1-H2)/2
 Y11=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-bf","5","7","2"
"        R-tw","1","11","0.3H"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","5","-2"
"        L-tf","8","7","1"
  
 Tessellation
 5
        1,2,10,11
        2,3,9,10
        4,5,6,3
        3,6,9
        9,6,7,8
  
 Line Data
 <Line Notation>
 4             5 
  
 Line X Data
        X1=0
        X2=B1/2
        X3=B1
        X4=B1/2
        X5=B1/2
  
 Line Y Data
        Y1=H1-H2/2
        Y2=H1-H2/2
        Y3=H1-H2/2
        Y4=H1/2
        Y5=0
  
 Line Thickness
 2
        T1=B2
        T2=H2
  
 Line Connectivity Data
 <Conectivity Notation>
"        1","2","T2"
"        2","3","T2"
"        2","4","T1"
"        4","5","T1"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Channel Shape
  Category = Cross Section
  Basic Shape Type = Channel
  Sub Shape Type = Channel
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 2
 Nh = 2
 Ncord = 14
  
 Path Data
 1             14            1 
  
 Horizontal Data
 B1=24
 B2=6
  
 Vertical Data
 H1=36
 H2=8
  
 X Data
 X1=0
 X2=0
 X3=0
 X4=B1/2
 X5=B1
 X6=B1
 X7=B2+(B1-B2)/2
 X8=B2
 X9=B2
 X10=B2
 X11=B2+(B1-B2)/2
 X12=B1
 X13=B1
 X14=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1
 Y5=H1
 Y6=H1-H2
 Y7=H1-H2
 Y8=H1-H2
 Y9=H1/2
 Y10=H2
 Y11=H2
 Y12=H2
 Y13=0
 Y14=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-bf","1","13","2"
"        R-tw","3","8","0.5H"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","3","-2"
"        R-tf","5","6","1"
  
 Tessellation
 6
        1,2,9,10
        2,3,8,9
        3,4,7,8
        4,5,6,7
        1,10,11,14
        14,11,12,13
  
 Line Data
 <Line Notation>
 6             7 
  
 Line X Data
        X1=B1
        X2=B1/2
        X3=B2/2
        X4=B2/2
        X5=B2/2
        X6=B1/2
        X7=B1
  
 Line Y Data
        Y1=H2/2
        Y2=H2/2
        Y3=H2/2
        Y4=H1/2
        Y5=H1-H2/2
        Y6=H1-H2/2
        Y7=H1-H2/2
  
 Line Thickness
 2
        T1=B2
        T2=H2
  
 Line Connectivity Data
 <Conectivity Notation>
"        1","2","T2"
"        2","3","T2"
"        3","4","T1"
"        4","5","T1"
"        5","6","T2"
"        6","7","T2"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE

 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = I Shape
  Category = Cross section
  Basic Shape Type = Flanged
  Sub Shape Type = I General
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 3
 Nh = 3
 Ncord = 16
  
 Path Data
 1             16            1 
  
 Horizontal Data
 B1=24
 B2=12
 B3=6
  
 Vertical Data
 H1=36
 H2=8
 H3=6
  
 X Data
 X1=B1/2-B2/2
 X2=B1/2-B2/2
 X3=B1/2-B3/2
 X4=B1/2-B3/2
 X5=B1/2-B3/2
 X6=0
 X7=0
 X8=B1/2-B3/2
 X9=B1/2+B3/2
 X10=B1
 X11=B1
 X12=B1/2+B3/2
 X13=B1/2+B3/2
 X14=B1/2+B3/2
 X15=B1/2+B2/2
 X16=B1/2+B2/2
  
 Y Data
 Y1=0
 Y2=H3
 Y3=H3
 Y4=H2+(H1-H2-H3)/2
 Y5=H1-H2
 Y6=H1-H2
 Y7=H1
 Y8=H1
 Y9=H1
 Y10=H1
 Y11=H1-H2
 Y12=H1-H2
 Y13=H2+(H1-H2-H3)/2
 Y14=H3
 Y15=H3
 Y16=0
  
 Horizontal Dimension
<Dimension Notations>
"        C-bf1","7","10","1"
"        C-bf2","1","16","-1"
"        R-tw","3","14","0.5H"
  
 Vertical Dimension
<Dimension Notations>
"        C-h","1","7","-2"
"        L-tf1","10","11","1"
"        R-tf2","1","2","1"
  
 Tessellation
 3
        1,2,3,14,15,16
        3,4,5,12,13,14
        5/12
  
 Line Data
 <Line Notation>
 6             7 
  
 Line X Data
        X1=B1/2-B2/2
        X2=B1/2
        X3=B1/2+B2/2
        X4=B1/2
        X5=B1/2
        X6=0
        X7=B1
  
 Line Y Data
        Y1=H3/2
        Y2=H3/2
        Y3=H3/2
        Y4=H1/2
        Y5=H1-H2/2
        Y6=H1-H2/2
        Y7=H1-H2/2
  
 Line Thickness
 3
        T1=H3
        T2=B3
        T3=H2
  
 Line Connectivity Data
 <Conectivity Notation>
"        1","2","T1"
"        2","3","T1"
"        2","4","T2"
"        4","5","T2"
"        6","5","T3"
"        5","7","T3"
 Prop From Database=No
 Prop Database=None
 Prop Record No=0

  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE

 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Chamfered Rectangle
  Category = Cross section
  Basic Shape Type = Rectangular
  Sub Shape Type = Chamfer Rectangle
  Is Hollow = No
  Is Champher = Yes
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 2
 Nh = 2
 Ncord = 12
  
 Path Data
 1             12            1 
  
 Horizontal Data
 B1=48
 B2=6
  
 Vertical Data
 H1=36
 H2=6
  
 X Data
 X1=B2
 X2=0
 X3=0
 X4=0
 X5=B2
 X6=B1/2
 X7=B1-B2
 X8=B1
 X9=B1
 X10=B1
 X11=B1-B2
 X12=B1/2
  
 Y Data
 Y1=0
 Y2=H2
 Y3=H1/2
 Y4=H1-H2
 Y5=H1
 Y6=H1
 Y7=H1
 Y8=H1-H2
 Y9=H1/2
 Y10=H2
 Y11=0
 Y12=0
  
 Horizontal Dimension
<Dimension Notations>
"      C-b","2","8","-1"
"      R-cx","1","2","1"
  
 Vertical Dimension
<Dimension Notations>
"      C-h","1","5","-1"
"      R-cy","11","10","1"
  
 Tessellation
 3
      1,2,3,4,5
      1,5,6,7,11,12
      11,7,8,9,10
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Rounded Rectangle
  Category = Cross section
  Basic Shape Type = Rectangular
  Sub Shape Type = Rounded Rectangle
  Is Hollow = No
  Is Champher = Yes
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = Yes
  
 Control Data
 Np = 1
 Nb = 1
 Nh = 2
 Ncord = 24
  
 Path Data
 1             24            1 
  
 Horizontal Data
 B1=48
  
 Vertical Data
 H1=36
 H2=6
  
 X Data
 X1=0
 X2=0
 X3=0
 X4=H2-H2*0.924
 X5=H2-H2*0.707
 X6=H2-H2*0.383
 X7=H2
 X8=B1/2
 X9=B1-H2
 X10=B1-H2+H2*0.383
 X11=B1-H2+H2*0.707
 X12=B1-H2+H2*0.924
 X13=B1
 X14=B1
 X15=B1
 X16=B1-H2+H2*0.924
 X17=B1-H2+H2*0.707
 X18=B1-H2+H2*0.383
 X19=B1-H2
 X20=B1/2
 X21=H2
 X22=H2-H2*0.383
 X23=H2-H2*0.707
 X24=H2-H2*0.924
  
 Y Data
 Y1=H2
 Y2=H1/2
 Y3=H1-H2
 Y4=H1-H2+H2*0.383
 Y5=H1-H2+H2*0.707
 Y6=H1-H2+H2*0.924
 Y7=H1
 Y8=H1
 Y9=H1
 Y10=H1-H2+H2*0.924
 Y11=H1-H2+H2*0.707
 Y12=H1-H2+H2*0.383
 Y13=H1-H2
 Y14=H1/2
 Y15=H2
 Y16=H2-H2*0.383
 Y17=H2-H2*0.707
 Y18=H2-H2*0.924
 Y19=0
 Y20=0
 Y21=0
 Y22=H2-H2*0.924
 Y23=H2-H2*0.707
 Y24=H2-H2*0.383
  
 Horizontal Dimension
<Dimension Notations>
"      C-b","1","15","-1"
  
 Vertical Dimension
<Dimension Notations>
"      C-h","21","7","-1"
"      R-r","19","15","1"
  
 Tessellation
 3
      21,22,23,24,1/7
      7,8,9,19,20,21
      9/19
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = General Triangle 
  Category = Cross Section
  Basic Shape Type = Triangular
  Sub Shape Type = Triangle
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 2
 Nh = 1
 Ncord = 6
  
 Path Data
 1             6             1 
  
 Horizontal Data
 B1=36
 B2=12
  
 Vertical Data
 H1=36
  
 X Data
 X1=0
 X2=(B1+B2)/2
 X3=B1+B2
 X4=B1+B2/2
 X5=B1
 X6=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1/2
 Y5=0
 Y6=0
  
 Horizontal Dimension
<Dimension Notations>
"      C-b1","1","3","-1"
"      R-b2","5","3","-1"
  
 Vertical Dimension
<Dimension Notations>
"      C-h","1","3","-1"
  
 Tessellation
 1
      1,2,3,4,5,6
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Equal Sided Triangle
  Category = Cross section
  Basic Shape Type = Triangular
  Sub Shape Type = Triangle
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 1
 Nh = 1
 Ncord = 6
  
 Path Data
 1             6             1 
  
 Horizontal Data
 B1=36
  
 Vertical Data
 H1=36
  
 X Data
 X1=0
 X2=B1/4
 X3=B1/2
 X4=3*B1/4
 X5=B1
 X6=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1/2
 Y5=0
 Y6=0
  
 Horizontal Dimension
<Dimension Notations>
"      C-b","1","5","-1"
  
 Vertical Dimension
<Dimension Notations>
"      C-h","1","3","-1"
  
 Tessellation
 1
      1,2,3,4,5,6
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE
 -------------------------------
 NEW SHAPE

 TYPE = ShapeGeneral
  Caption = Right Angle Triangle
  Category = Cross section
  Basic Shape Type = Triangular
  Sub Shape Type = Triangle
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = No
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = No
  
 Control Data
 Np = 1
 Nb = 1
 Nh = 1
 Ncord = 6
  
 Path Data
 1             6             1 
  
 Horizontal Data
 B1=36
  
 Vertical Data
 H1=36
  
 X Data
 X1=0
 X2=0
 X3=0
 X4=B1/2
 X5=B1
 X6=B1/2
  
 Y Data
 Y1=0
 Y2=H1/2
 Y3=H1
 Y4=H1/2
 Y5=0
 Y6=0
  
 Horizontal Dimension
<Dimension Notations>
"      C-b","1","5","-1"
  
 Vertical Dimension
<Dimension Notations>
"      C-h","1","3","-1"
  
 Tessellation
 1
      1/6
 Prop From Database=No
 Prop Database=None
 Prop Record No=0
  
  
 TAG = 
 END TYPE = ShapeGeneral
 END SHAPE

 -------------------------------
 NEW SHAPE
 
 TYPE = ShapeGeneral
  Caption = Circle
  Category = Cross section
  Basic Shape Type = Circle
  Sub Shape Type = Circle
  Is Hollow = No
  Is Champher = No
  Is Fillet = No
  Is Variable Flange = No
  Is Inclined Web = No
  Is Lipped = No
  Is Symmetrical = Yes
  Is Builtup = No
  Use As Void = 0
  Main Material = Concrete 
  Sub Material = 
  Material Type = 0
  Units = US
  X0 = 0
  Y0 = 0
  Angle = 0
  MirrorOnX = 0
  MirrorOnY = 0
  Has Arcs = Yes

 Control Data
 Np=1
 Nb=1
 Nh=0
 Ncord=24

 Path Data
 1,24,1
 
Horizontal Data
 B1=36

 Vertical Data

 X Data
 X1=0
 X2=B1/2-B1/2*0.9659
 X3=B1/2-B1/2*0.8660
 X4=B1/2-B1/2*0.7071
 X5=B1/2-B1/2*0.5
 X6=B1/2-B1/2*0.2588
 X7=B1/2
 X8=B1/2+B1/2*0.2588
 X9=B1/2+B1/2*0.5
 X10=B1/2+B1/2*0.7071
 X11=B1/2+B1/2*0.8660
 X12=B1/2+B1/2*0.9659
 X13=B1/2+B1/2
 X14=B1/2+B1/2*0.9659
 X15=B1/2+B1/2*0.8660
 X16=B1/2+B1/2*0.7071
 X17=B1/2+B1/2*0.5
 X18=B1/2+B1/2*0.2588
 X19=B1/2
 X20=B1/2-B1/2*0.2588
 X21=B1/2-B1/2*0.5
 X22=B1/2-B1/2*0.7071
 X23=B1/2-B1/2*0.8660
 X24=B1/2-B1/2*0.9659

 Y Data
 Y1=B1/2
 Y2=B1/2+B1/2*0.2588
 Y3=B1/2+B1/2*0.5
 Y4=B1/2+B1/2*0.7071
 Y5=B1/2+B1/2*0.8660
 Y6=B1/2+B1/2*0.9659
 Y7=B1/2+B1/2
 Y8=B1/2+B1/2*0.9659
 Y9=B1/2+B1/2*0.8660
 Y10=B1/2+B1/2*0.7071
 Y11=B1/2+B1/2*0.5
 Y12=B1/2+B1/2*0.2588
 Y13=B1/2
 Y14=B1/2-B1/2*0.2588
 Y15=B1/2-B1/2*0.5
 Y16=B1/2-B1/2*0.7071
 Y17=B1/2-B1/2*0.8660
 Y18=B1/2-B1/2*0.9659
 Y19=0
 Y20=B1/2-B1/2*0.9659
 Y21=B1/2-B1/2*0.8660
 Y22=B1/2-B1/2*0.7071
 Y23=B1/2-B1/2*0.5
 Y24=B1/2-B1/2*0.2588

 Horizontal Dimension
"Dimension Name","First Pt", "Second Pt","Scal"
 "         C-t2","1","13","1"
 
 Vertical Dimension
"Dimension Name","First Pt", "Second Pt","Scal"

 Tessellation
 1
 1/24

 Prop From Database=No
 Prop Database=None
 Prop Record No=0


 END SHAPE

 -------------------------------
